# SC-F001 project-level sdkconfig overrides.
# These are applied during "idf.py reconfigure" and take precedence over IDF defaults.
# Do NOT override settings that are managed by idf.py menuconfig interactively.

# 32kHz external crystal (GPIO32/33) is on the PCB but NOT used.
# Deep sleep is disabled (soft idle instead), so RTC slow clock accuracy is irrelevant.
# Time tracking uses esp_timer (40MHz APB crystal, ~20ppm).
# Let the RTC slow clock use the default internal RC oscillator.

# --- Safety & Panic ---

# WDT timeout triggers a panic (→ reboot + core dump) instead of just logging.
# Required for OTA rollback: a hung task causes a reboot, incrementing the reset counter.
CONFIG_ESP_TASK_WDT_PANIC=y
