[1/5] cmd.exe /C "cd /D C:\data\stockcropper-sw-playground\SC-F001\build\esp-idf\esptool_py && C:\Espressif\python_env\idf5.3_py3.11_env\Scripts\python.exe C:/Espressif/frameworks/esp-idf-v5.3.1/components/partition_table/check_sizes.py --offset 0x8000 partition --type app C:/data/stockcropper-sw-playground/SC-F001/build/partition_table/partition-table.bin C:/data/stockcropper-sw-playground/SC-F001/build/app-template.bin"
app-template.bin binary size 0x32350 bytes. Smallest app partition is 0x200000 bytes. 0x1cdcb0 bytes (90%) free.

[2/5] Performing build step for 'bootloader'
[1/1] cmd.exe /C "cd /D C:\data\stockcropper-sw-playground\SC-F001\build\bootloader\esp-idf\esptool_py && C:\Espressif\python_env\idf5.3_py3.11_env\Scripts\python.exe C:/Espressif/frameworks/esp-idf-v5.3.1/components/partition_table/check_sizes.py --offset 0x8000 bootloader 0x1000 C:/data/stockcropper-sw-playground/SC-F001/build/bootloader/bootloader.bin"

Bootloader binary size 0x6880 bytes. 0x780 bytes (7%) free.


[2/3] cmd.exe /C "cd /D C:\Espressif\frameworks\esp-idf-v5.3.1\components\esptool_py && C:\Espressif\tools\cmake\3.24.0\bin\cmake.exe -D IDF_PATH=C:/Espressif/frameworks/esp-idf-v5.3.1 -D SERIAL_TOOL=C:/Espressif/python_env/idf5.3_py3.11_env/Scripts/python.exe;;C:/Espressif/frameworks/esp-idf-v5.3.1/components/esptool_py/esptool/esptool.py;--chip;esp32 -D SERIAL_TOOL_ARGS=--before=default_reset;--after=hard_reset;write_flash;@flash_args -D WORKING_DIRECTORY=C:/data/stockcropper-sw-playground/SC-F001/build -P C:/Espressif/fraesptool.py --chip esp32 -p COM3 -b 460800 --before=default_reset --after=hard_reset write_flash --flash_mode dio --flash_freq 40m --flash_size 8MB 0x1000 bootloader/bootloader.bin 0x10000 app-template.bin 0x8000 partition_table/partition-table.bin 0xd000 ota_data_initial.bin
esptool.py v4.8.1
Serial port COM3
Connecting....
Chip is ESP32-D0WD-V3 (revision v3.1)
Features: WiFi, BT, Dual Core, 240MHz, VRef calibration in efuse, Coding Scheme None
Crystal is 40MHz
MAC: 94:54:c5:38:c4:38
Uploading stub...
Running stub...
Stub running...
Changing baud rate to 460800
Changed.
Configuring flash size...
Flash will be erased from 0x00001000 to 0x00007fff...
Flash will be erased from 0x00010000 to 0x00042fff...
Flash will be erased from 0x00008000 to 0x00008fff...
Flash will be erased from 0x0000d000 to 0x0000efff...
SHA digest in image updated
Compressed 26752 bytes to 16359...
Writing at 0x00001000... (100 %)
Wrote 26752 bytes (16359 compressed) at 0x00001000 in 0.6 seconds (effective 383.4 kbit/s)...
Hash of data verified.
Compressed 205648 bytes to 110327...
Writing at 0x00010000... (14 %)
Writing at 0x0001cf4d... (28 %)
Writing at 0x00022f87... (42 %)
Writing at 0x00028c81... (57 %)
Writing at 0x0002f889... (71 %)
Writing at 0x00037936... (85 %)
Writing at 0x0003d98f... (100 %)
Wrote 205648 bytes (110327 compressed) at 0x00010000 in 2.7 seconds (effective 608.8 kbit/s)...
Hash of data verified.
Compressed 3072 bytes to 143...
Writing at 0x00008000... (100 %)
Wrote 3072 bytes (143 compressed) at 0x00008000 in 0.0 seconds (effective 957.1 kbit/s)...
Hash of data verified.
Compressed 8192 bytes to 31...
Writing at 0x0000d000... (100 %)
Wrote 8192 bytes (31 compressed) at 0x0000d000 in 0.0 seconds (effective 2039.1 kbit/s)...
Hash of data verified.

Leaving...
Hard resetting via RTS pin...
meworks/esp-idf-v5.3.1/components/esptool_py/run_serial_tool.cmake"
