[1/5] cmd.exe /C "cd /D C:\data\stockcropper-sw-playground\SC-F001\build\esp-idf\esptool_py && C:\Espressif\python_env\idf5.3_py3.11_env\Scripts\python.exe C:/Espressif/frameworks/esp-idf-v5.3.1/components/partition_table/check_sizes.py --offset 0x8000 partition --type app C:/data/stockcropper-sw-playground/SC-F001/build/partition_table/partition-table.bin C:/data/stockcropper-sw-playground/SC-F001/build/app-template.bin"
app-template.bin binary size 0x32400 bytes. Smallest app partition is 0x200000 bytes. 0x1cdc00 bytes (90%) free.

[2/5] Performing build step for 'bootloader'
[1/1] cmd.exe /C "cd /D C:\data\stockcropper-sw-playground\SC-F001\build\bootloader\esp-idf\esptool_py && C:\Espressif\python_env\idf5.3_py3.11_env\Scripts\python.exe C:/Espressif/frameworks/esp-idf-v5.3.1/components/partition_table/check_sizes.py --offset 0x8000 bootloader 0x1000 C:/data/stockcropper-sw-playground/SC-F001/build/bootloader/bootloader.bin"

Bootloader binary size 0x6880 bytes. 0x780 bytes (7%) free.


[2/3] cmd.exe /C "cd /D C:\Espressif\frameworks\esp-idf-v5.3.1\components\esptool_py && C:\Espressif\tools\cmake\3.24.0\bin\cmake.exe -D IDF_PATH=C:/Espressif/frameworks/esp-idf-v5.3.1 -D SERIAL_TOOL=C:/Espressif/python_env/idf5.3_py3.11_env/Scripts/python.exe;;C:/Espressif/frameworks/esp-idf-v5.3.1/components/esptool_py/esptool/esptool.py;--chip;esp32 -D SERIAL_TOOL_ARGS=--before=default_reset;--after=hard_reset;write_flash;@flash_args -D WORKING_DIRECTORY=C:/data/stockcropper-sw-playground/SC-F001/build -P C:/Espressif/fraesptool.py --chip esp32 -p COM3 -b 460800 --before=default_reset --after=hard_reset write_flash --flash_mode dio --flash_freq 40m --flash_size 8MB 0x1000 bootloader/bootloader.bin 0x10000 app-template.bin 0x8000 partition_table/partition-table.bin 0xd000 ota_data_initial.bin
esptool.py v4.8.1
Serial port COM3
Connecting....
Chip is ESP32-D0WD-V3 (revision v3.1)
Features: WiFi, BT, Dual Core, 240MHz, VRef calibration in efuse, Coding Scheme None
Crystal is 40MHz
MAC: 94:54:c5:38:c4:38
Uploading stub...
Running stub...
Stub running...
Changing baud rate to 460800
Changed.
Configuring flash size...
Flash will be erased from 0x00001000 to 0x00007fff...
Flash will be erased from 0x00010000 to 0x00042fff...
Flash will be erased from 0x00008000 to 0x00008fff...
Flash will be erased from 0x0000d000 to 0x0000efff...
SHA digest in image updated
Compressed 26752 bytes to 16359...
Writing at 0x00001000... (100 %)
Wrote 26752 bytes (16359 compressed) at 0x00001000 in 0.6 seconds (effective 383.4 kbit/s)...
Hash of data verified.
Compressed 205824 bytes to 110451...
Writing at 0x00010000... (14 %)
Writing at 0x0001cf3b... (28 %)
Writing at 0x00022fad... (42 %)
Writing at 0x00028ca0... (57 %)
Writing at 0x0002f8a4... (71 %)
Writing at 0x00037936... (85 %)
Writing at 0x0003d93c... (100 %)
Wrote 205824 bytes (110451 compressed) at 0x00010000 in 2.7 seconds (effective 610.5 kbit/s)...
Hash of data verified.
Compressed 3072 bytes to 142...
Writing at 0x00008000... (100 %)
Wrote 3072 bytes (142 compressed) at 0x00008000 in 0.0 seconds (effective 944.3 kbit/s)...
Hash of data verified.
Compressed 8192 bytes to 31...
Writing at 0x0000d000... (100 %)
Wrote 8192 bytes (31 compressed) at 0x0000d000 in 0.0 seconds (effective 1798.0 kbit/s)...
Hash of data verified.

Leaving...
Hard resetting via RTS pin...
meworks/esp-idf-v5.3.1/components/esptool_py/run_serial_tool.cmake"
