[1/5] cmd.exe /C "cd /D C:\data\stockcropper-sw-playground\SC-F001\build\esp-idf\esptool_py && C:\Espressif\python_env\idf5.3_py3.11_env\Scripts\python.exe C:/Espressif/frameworks/esp-idf-v5.3.1/components/partition_table/check_sizes.py --offset 0x8000 partition --type app C:/data/stockcropper-sw-playground/SC-F001/build/partition_table/partition-table.bin C:/data/stockcropper-sw-playground/SC-F001/build/app-template.bin"
app-template.bin binary size 0x323d0 bytes. Smallest app partition is 0x200000 bytes. 0x1cdc30 bytes (90%) free.

[2/5] Performing build step for 'bootloader'
[1/1] cmd.exe /C "cd /D C:\data\stockcropper-sw-playground\SC-F001\build\bootloader\esp-idf\esptool_py && C:\Espressif\python_env\idf5.3_py3.11_env\Scripts\python.exe C:/Espressif/frameworks/esp-idf-v5.3.1/components/partition_table/check_sizes.py --offset 0x8000 bootloader 0x1000 C:/data/stockcropper-sw-playground/SC-F001/build/bootloader/bootloader.bin"

Bootloader binary size 0x6880 bytes. 0x780 bytes (7%) free.


[2/3] cmd.exe /C "cd /D C:\Espressif\frameworks\esp-idf-v5.3.1\components\esptool_py && C:\Espressif\tools\cmake\3.24.0\bin\cmake.exe -D IDF_PATH=C:/Espressif/frameworks/esp-idf-v5.3.1 -D SERIAL_TOOL=C:/Espressif/python_env/idf5.3_py3.11_env/Scripts/python.exe;;C:/Espressif/frameworks/esp-idf-v5.3.1/components/esptool_py/esptool/esptool.py;--chip;esp32 -D SERIAL_TOOL_ARGS=--before=default_reset;--after=hard_reset;write_flash;@flash_args -D WORKING_DIRECTORY=C:/data/stockcropper-sw-playground/SC-F001/build -P C:/Espressif/fraesptool.py --chip esp32 -p COM3 -b 460800 --before=default_reset --after=hard_reset write_flash --flash_mode dio --flash_freq 40m --flash_size 8MB 0x1000 bootloader/bootloader.bin 0x10000 app-template.bin 0x8000 partition_table/partition-table.bin 0xd000 ota_data_initial.bin
esptool.py v4.8.1
Serial port COM3
Connecting......
Chip is ESP32-D0WD-V3 (revision v3.1)
Features: WiFi, BT, Dual Core, 240MHz, VRef calibration in efuse, Coding Scheme None
Crystal is 40MHz
MAC: 94:54:c5:38:c4:38
Uploading stub...
Running stub...
Stub running...
Changing baud rate to 460800
Changed.
Configuring flash size...
Flash will be erased from 0x00001000 to 0x00007fff...
Flash will be erased from 0x00010000 to 0x00042fff...
Flash will be erased from 0x00008000 to 0x00008fff...
Flash will be erased from 0x0000d000 to 0x0000efff...
SHA digest in image updated
Compressed 26752 bytes to 16359...
Writing at 0x00001000... (100 %)
Wrote 26752 bytes (16359 compressed) at 0x00001000 in 0.6 seconds (effective 384.5 kbit/s)...
Hash of data verified.
Compressed 205776 bytes to 110402...
Writing at 0x00010000... (14 %)
Writing at 0x0001cf68... (28 %)
Writing at 0x00022fb6... (42 %)
Writing at 0x00028c94... (57 %)
Writing at 0x0002f8cc... (71 %)
Writing at 0x0003794a... (85 %)
Writing at 0x0003d967... (100 %)
Wrote 205776 bytes (110402 compressed) at 0x00010000 in 2.7 seconds (effective 610.8 kbit/s)...
Hash of data verified.
Compressed 3072 bytes to 142...
Writing at 0x00008000... (100 %)
Wrote 3072 bytes (142 compressed) at 0x00008000 in 0.0 seconds (effective 916.4 kbit/s)...
Hash of data verified.
Compressed 8192 bytes to 31...
Writing at 0x0000d000... (100 %)
Wrote 8192 bytes (31 compressed) at 0x0000d000 in 0.0 seconds (effective 2111.0 kbit/s)...
Hash of data verified.

Leaving...
Hard resetting via RTS pin...
meworks/esp-idf-v5.3.1/components/esptool_py/run_serial_tool.cmake"
